Sound device with QFM for T98-Next (Modified SoundSPB.nhw)

Emulate Speak Board (Only QFM+LPF)

FM      ok
SSG     ok
RHYTHM  ok
ADPCM	ok
CSM		ok
SSGPCM	ok (but...)
86PCM	non support
WSS		non support

ROMEO	ok?

You must be restarted after changing the configuration

If you want to use external FM synth engine (dll)
Put dll file in the Next folder.
Adding FMGenDll= line to [SpindSPB] section of MAIN.INI
Need reexecute

Update & fixed:

Apr 07,2012
	Support to SSGPCM
	Support to FMGenDll
	and few bugs fixed

Sep 08,2011
	Rate listbox 88100 to 88200
	Uses MMX and SSE2, if available
	and etc...

Sep 13,2011
	ADPCM Rate
	Reflected volume without restarting
	